# SEGA Dreamcast Specifications

### CPU Specifications:
- **Processor**:								Hitachi SH-4 (128-bit)
- **Processor Speed**:							200 MHz
- **Millions of instructions per second**:		360
- **Floating-point operations per seccond**:	1.4 billion
- **Main RAM**:									16MB SDRAM

### GPU Specifications:
- **Processor**:				NEC PowerVR2 DC
- **Polygons per second**:		7.0 Million
- **Video RAM**:				8 MiB 4x16 Bit
- **Fillrate**:					100 MPixels/s

### Audio Specifications:
- **Processor**:				Yamaha AICA (32-bit)
- **Processor Speed**:			22.5 MHz
- **Co-Processor**:				ARM7 RISC
- **Co-Processor Speed**:		45 MHz
- **Channels**:					64
- **Audio RAM**:				2 MiB (16-bit)
